Effect of supplementary irrigation water and organic matter amounts on tomato yield and water productivity in a semi-arid climate

.

ABSTRACT

|  |
| --- |
|  |
| Although promoted as an alternative to secure rain-fed agriculture, supplementary irrigation cannot ensure sustainable food production, regardless of the rational and optimal use of organic matter. Therefore, an experiment was set up to determine the optimal combination of irrigation depth and compost rate. The experimental design was a split plot with four replications. The main factor was the irrigation water depths, which represented 50%, 75%, and 100% of the tomato crop’s water requirement. The second factor consisted of two compost rates: 5 t/ha (C5) and 10 t/ha (C10). Six combinations were tested: C10 + 100%, C10 + 75%, C10 + 50%, C5 + 100%, C5 + 75%, and C5 + 50%. The compost was applied during land preparation. Fertilizers (NPK 14-23-14 and Urea 46%) were applied at the recommended rates of 250 kg/ha and 150 kg/ha, respectively, at 15 and 35 days after transplanting. The adopted irrigation interval was 2 days. After transplanting, a constant water depth (DI 100%) was applied, and water treatments were initiated 15 days after transplanting. Water application was postponed to the next irrigation if rain occurred.  The results showed that, in general under supplementary irrigation, the addition of compost increase growth parameters, yield and water use productivity. However, when water requirement is reduced by half this increase is not consistent. Indeed, the higher yield was induced by C5 + 75% treatment. The combination of C10 + 50% improved water productivity by 70%. Therefore, the combination of C10 + 50% should be recommended for the sustainable management of land and water resources. |

*Keywords: supplementary irrigation, sustainable management of land and water, tomato, Burkina Faso*

1. INTRODUCTION

Tomato (*Solanum lycopersicum* L.) is one of the most widely cultivated crops globally. According to [1], [2] approximately 18 billion tons of tomatoes are produced annually. In Burkina Faso, tomatoes are among the most important vegetables produced during both the dry and rainy seasons [3] In Ouagadougou, tomatoes, alongside other vegetables, account for 80% of the local demand for vegetables and fruits. Their production provides employment, with around a hundred sites in the Kossodo area [4]. However, tomatoes are among the most water-demanding crops [5]. Excessive water application negatively affects the nutrient content of the crop [6], [7] and increases humidity, either in the atmosphere or in greenhouses, thus facilitating the spread of diseases and pests. Furthermore, over-irrigation leads to the leaching of soil nutrients and pesticides [8]. Conversely, water deficits can hinder plant development and significantly reduce yields [9], [10], [11], [12]. These studies have further suggested that tomatoes can develop adaptive mechanisms, such as reducing photosynthesis, under severe water stress.

Numerous researchers have studied the role of organic amendments in enhancing soil productivity. Findings indicate that these amendments improve soil quality, structure, nutrient availability, and overall plant productivity [13] . Organic amendments perform several functions, including nutrient storage and gradual release through mineralization, which helps meet the nutritional needs of plants. Additionally, they contribute to soil structuring and stability, protecting it from external threats such as water erosion. Organic amendments also stimulate biological activity, enhance soil aeration, and improve water retention capacity, which can reduce the frequency and volume of irrigation required. This water retention function is becoming increasingly important as it is viewed as an integrated approach to soil management, thus promoting agricultural production. When the application of organic matter is combined with supplemental irrigation, this approach offers a viable solution to challenges such as drought conditions and soil impoverishment [14]. The optimal application of supplemental irrigation paired with organic matter has the potential to significantly reduce irrigation water requirements while improving soil productivity.

Several studies have examined the synergy between organic amendments and irrigation levels in crop growth and yield. For instance, [15] observed that organic amendments stimulate spinach growth; however, this improvement was not significant under deficient irrigation. [16] recommended using low levels of organic amendments to mitigate the adverse effects of drought on spinach growth and yield. [17] concluded that integrated fertilization systems are more reliable than conventional systems for producing high-quality forage barley in arid environments, especially under late-stage water stress or deficit irrigation systems.

The responses of crops and soils to organic amendments and irrigation strategies depend on multiple factors, such as soil type, crop species, soil chemistry, and climatic conditions. Moreover, many producers apply organic matter either in excess or insufficient amounts, often combined with poorly managed irrigation practices. These situations lead to resource wastage and reduced agricultural productivity. It is essential, therefore, to assess the effectiveness of these techniques, particularly for water-intensive crops in arid regions characterized by nutrient-poor soils.

This study aims to enhance both soil and water productivity through a synergistic approach that combines water management and organic matter application (compost) in tomato cultivation. An experimental trial was conducted on a site with tomato crops, employing three irrigation regimes:

* Full irrigation, meeting 100% of the tomato's water requirements,
* Recommended irrigation, covering 75% of the crop's water requirements, and
* Reduced irrigation, covering 50% of the crop's water needs.

Each irrigation treatment was combined with three organic matter application rates: 0 t/ha, 5 t/ha, and 10 t/ha. The tomato plants’ morphological parameters were monitored throughout the trial, while water productivity and yield were evaluated at harvest. Soil samples were collected before and after the trial to measure the treatment effect on soil microbial activity.

2. material and methods

2.1. Location

The study was conducted from May 3 to July 10, 2023, at an experimental site located within the premises of IPD-AOS in Ouagadougou, Burkina Faso, at coordinates 12°23'N, 1°28'W, and an altitude of 294 meters. The climate at the study site is classified as dry tropical, within the Sudanian-Sahelian zone. The region is characterized by a dry season, lasting six to eight months (from November to May), dominated by dry winds from the Sahara, and a rainy season, spanning four to five months (from June to September), dominated by humid winds from the Gulf of Guinea. On average, the area receives between 600 and 900 mm of rainfall annually, and the terrain is predominantly flat. The highest temperatures are recorded in April and May, reaching up to 43°C, while the lowest temperatures are recorded in December and January, with temperatures dropping as low as 16°C. The hydrographic network, including numerous wells and boreholes, facilitates the use of surface and groundwater for crop irrigation during the dry season.

2.2. **The plant material used**

The tomato varieties used in the experiments were Tropimech Tri Active Blue and Cobra 26 F1. These are among the most commonly cultivated varieties in Burkina Faso and are well-suited for the rainy season. The Tropimech Tri Active Blue variety produces firm, elongated fruits weighing between 90 and 100 grams at maturity. It has an average production period of 65 to 70 days after transplanting and offers excellent shelf life. Similarly, the Cobra 26 F1 variety yields firm fruits with uniform coloration, weighing between 80 and 90 grams. Its average production period is approximately 65 days after transplanting, and it also has a long shelf life. These characteristics make both varieties ideal for local agricultural practices and market demands.

2.3. **The experimental design**

The experimental design employed was a split-plot design with four replications and nine treatments. The primary factor was the irrigation dosage, while the secondary factor was the organic matter dosage. Each block consisted of three main plots, each corresponding to one of the three primary irrigation levels. These main plots were subdivided into three subplots, each representing one of the three organic matter application rates. This resulted in nine subplots per block and a total of 36 subplots across the entire experiment.

Each subplot measured 2 meters in length and 2 meters in width, covering an area of 4 square meters, and contained five furrows. Six tomato planting holes (poquets) were established per furrow, resulting in a total of 30 planting holes per subplot. Blocks were separated by a 1-meter distance, while subplots within each block were spaced 0.5 meters apart. The total experimental area covered 264 square meters.

Each treatment was a combination of an irrigation dosage and an organic matter dosage. Initially, compost was applied to the soil at rates of 0 t/ha, 5 t/ha, and 10 t/ha, corresponding to 0, 2, and 4 kilograms of compost per subplot, respectively. Irrigation water was then applied at field capacity levels of 100%, 75%, and 50%, corresponding to 3, 2, and 1 watering cans per furrow, equating to 32, 24, and 12 liters per furrow, respectively.

The treatments were as follows:

* **C0 + 100%**: 100% irrigation and no organic matter;
* **C5 + 100%**: 100% irrigation and 5 t/ha organic matter;
* **C10 + 100%**: 100% irrigation and 10 t/ha organic matter;
* **C0 + 75%**: 75% irrigation and no organic matter;
* **C5 + 75%**: 75% irrigation and 5 t/ha organic matter;
* **C10 + 75%**: 75% irrigation and 10 t/ha organic matter;
* **C0 + 50%**: 50% irrigation and no organic matter;
* **C5 + 50%**: 50% irrigation and 5 t/ha organic matter;
* **C10 + 50%**: 50% irrigation and 10 t/ha organic matter.

The corresponding irrigation treatments were applied 15 days after transplanting (15 DAT) and continued every two days until harvest, except on rainy days.

**2.3. TRIAL IMPLEMENTATION**

The experiment was conducted over two consecutive years. During both the first and second years, after the application of compost, tomato plants were transplanted at a density of six plants per row, with a spacing of 0.4 m between plants, resulting in 30 plants per experimental plot. The plants were irrigated daily for 15 days, with 12 liters of water per row per day. After this initial period, 250 kg/ha of NPK fertilizer was applied, and the different irrigation treatments started. Irrigation was subsequently applied every two days, except during rainfall. Then after 35 DAT urea (46% N) was applied 35 days after transplanting

Chemical pesticide treatments were applied annually to address and prevent plant diseases from developing within the experimental setup.

**2.4. Observations and Measured Parameters**

**2.4.1. Morphological Parameters**

Morphological parameters were assessed at 15, and 35 days after transplanting (DAT). Observations were made on ten plants per experimental plot, selected alternately to ensure representative sampling. The parameters measured included:

* Plant height: Measured from the base to the topmost leaf using a graduated measuring tape.
* Stem diameter: Determined using a caliper at the collar of the plant.
* Number of leaves: Counted manually.

**2.4.2. Production Parameters**

After each harvest, the following parameters were recorded for the ten selected plants per plot:

* Number of fruits per plant: Counted for each of the selected plants.
* Fruit dimensions: Length and diameter measured with a caliper.
* Fruit weight: Assessed using a precision balance.

The yield was calculated using the formula:

R(kg/ha)=P(kg)×41600

Where:

R: Yield (kg/ha)

P: Average weight of fruits per plot

**2.4.3. Water Use Efficiency**

Water use productivity was determined using [18]equations for:

Water use efficiency

: The yield

**:** Water quantity used for the irrigation of the plot

**2.5. Data Processing and Statistical Analysis**

Data entry was performed using Microsoft Excel 2017. The collected data were analyzed through analysis of variance (ANOVA) using SPSS software version 21. For comparing treatment means, the Newman-Keuls test was employed when ANOVA indicated statistically significant differences at the 5% significance level.

3. results and discussion

3.1. Results

3.1.1. Climate data

Figure 1 below shows monthly rainfall, effective rainfall, and temperatures from May to October for both years of experimentation. The results indicate that during the period from May to October, the second year of the experiment recorded 32% more precipitation and a 14% increase in effective rainfall compared to the first year of the experiment. Moreover, the lowest and highest temperatures were recorded during the second year of the experiment.

Figure. 1. Monthly rainfall, effective rainfall, maximum and minimum temperature for 2023 et 2024 years of study area

3.1.2. Effect of supplementary irrigation dose and organic matter dose on tomato growth parameters

3.1.2.1. Plant Hight

Table 3 presents the results of the effects of treatments on the Hight of tomato plants over two years of experimentation for 15 DAT and 25 DAT. Statistical analysis revealed no significant impact of treatments on plant hight at any growth stage, despite the application of compost. However, the tallest plants were consistently recorded in the C10+75% plot during both years, while the shortest plants were observed in the C5+50% plot. Additionally, tomato plants showed greater growth in the second year compared to the first. These findings indicate that, aside from the C5+50% and C10+75% treatments, which produced the shortest and tallest plants respectively, the treatments resulted in similar plant heights regardless of the addition of organic matter.

**Table 1. Effect of treatment on plants Height at 15 and 25 DAT during the first and the second year of experimentation**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| treatment | Hight1(15 DAT) | Hight2(15 DAT) | Average | Hight1(25 DAT) | Hight2(25 DAT) | Average |
| C10 + 100% | 23,81± 1,30 | 24,82±1,06 | 24,32±0,84 | 34,54± 1,83 | 46,40±2,34 | 40,47±1,62 |
| C5+ 100% | 22,85± 1,94 | 25,42±0,95 | 24,14±1,09 | 31,66± 1,72 | 46,46±1,69a | 39,06±1,46 |
| CO + 100% | 24,41± 1,32 | 25,45±0,87 | 24,94±0,79 | 33,90± 1,66 | 48,57±1,84a | 41,24±1,48 |
| C10+ 75% | 25,63± 1,30 | 26,27±0,91 | 25,96±0,79 | 36,41± 1,56 | 51,00±1,81 | 43,8±1,45 |
| C5 + 75% | 23,82± 1,14 | 23,08±0,77 | 23,46±0,69 | 34,43± 1,47 | 43,83±1,80 | 39,13±1,27 |
| CO + 75% | 23,84± 1,10 | 23,41±0,91 | 23,63±0,71 | 33,31± 1,66 | 44,69±1,42 | 39,01±1,26 |
| C10 + 50% | 23,81± 1,12 | 25,44±0,97 | 24,63±0,75 | 32,38± 1,64 | 46,48±1,76 | 39,43±1,44 |
| C5 +50% | 23,14± 1,02 | 23,26±0,83 | 23,21±0,66 | 31,81± 1,53 | 45,03±2,04 | 38,43±1,47 |
| CO + 50% | 23,43± 1,04 | 23,25±1,0,3 | 23,34±0,73 | 34,02± 1,33 | 42,70±1,92 | 38,36±1,26 |
| Probability | 0,92 | 0,86 | 0,252 | 0,54 | 0,075 | 0,156 |
| Signification | ns | ns | ns | ns | ns | ns |

*ns means no significant*

*Hight1 (15 DAT) means the hight of plant in the first year of experimentation at 15 days after transplanting.*

*HIGHT2 (15 DAT) means the hight of plant in the second year of experimentation at 15 days after transplanting.*

*Hight1 (25 DAT) means the Hight of plant in the first year of experimentation at 25 days after transplanting.*

*Hight2 (25 DAT) means the hight of plant in the second year of experimentation at 25 days after transplanting.*

3.1.2.2. Stem diameter

Table 2 illustrates the effect of different treatments on the stem diameter of tomato plants over two years of experimentation. Statistical analysis revealed that treatments significantly influenced stem diameter at 25 days after transplanting (DAT). The application of organic matter demonstrated varying effects across irrigation levels. At the D100% irrigation level, applying 10 t/ha of organic matter resulted in a significant 9% increase in stem diameter compared to the average of the C0+D100% and C5+D100% treatments. Similarly, at the D75% level, a 10 t/ha organic matter application led to an 11% increase in stem diameter compared to the C0+D75% treatment. In contrast, no significant effect was observed at the D50% irrigation level for applications of 5 and 10 t/ha of organic matter. Additionally, plants from the first year of experimentation generally exhibited larger stem diameters than those from the second year. These findings suggest that in supplementary irrigation conditions, the growth phase and the application of 10 t/ha of organic matter significantly influence the stem diameter of tomato plants.

**Table 2. Effect of treatment on stem diameter at 15 and 25 DAT during the first and the second year of experimentation**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Treatment** | **S. diameter1(15 DAT)** | **S. diameter2(15 DAT)** | **Average** | **S. diameter1(25 DAT)** | **S. diameter2(25 DAT)** | **Average** |
| C10 + 100% | 5,13± 0,197 | 3,87±0,15a | 4,51±0,14 | 6,38±0,19abc | 6,15±0,26a | 6,27±0,16a |
| C5 + 100% | 4,56± 0,27 | 3,72±0,12a | 4,15±0,16 | 5,72±0,2abc | 5,60±0,15ab | 5,67±0,13ab |
| C0+ 100% | 4,57± 0,15 | 3,61±0,13a | 4,09±0,11 | 6,02±0,22abc | 5,62±0,15ab | 5,82±0,13ab |
| C10+ 75% | 5,04± 0,16 | 3,71±0,12a | 4,38±0,13 | 6,49±0,19a | 5,98±0,18a | 6,23±0,14a |
| C5 + 75% | 5,18±0,18 | 3,64±0,11a | 4,42±0,14 | 6,19±0,28abc | 5,14±0,20b | 5,67±0,18ab |
| C0 + 75% | 4,73± 0,15 | 3,48 ±0,11ab | 4,11±0,12 | 5,78±0,23abc | 3,39±0,15b | 5,59±0,14b |
| C10 + 50% | 4,66± 0,20 | 3,55±0,10ab | 4,11±0,13 | 5,39±0,3abc | 5,65±0,14ab | 5,52±0,16b |
| C5 +50% | 4,54± 0,17 | 3,18±0,15bc | 3,8±0,13 | 5,13±0,21c | 5,37±0,18b | 5,25±0,14b |
| C0+ 50% | 6,54± 2,12 | 2,59 ±0,14c | 4,75±1,08 | 5,59±0,18abc | 5,35±0,17b | 5,47±0,13b |
| Probability | 0,64 | 0 | 0,8 | 0 | 0,003 | 0 |
| Signification | ns | \*\*\* | ns | \*\*\* | \*\* | \*\*\* |

*ns means no significant*

*\*\*\* means significant when P˂ 0,001*

*\*\* means significant when P˂ 0,005*

***S. diameter****1(15 DAT) means the stem diameter of plant in the first year of experimentation at 15 days after transplanting*

***S. diameter*** *2(15 DAT) means the stem diameter of plant in the second year of experimentation at 15 days after transplanting*

***S. diameter****1(25 DAT) means the stem diameter of plant in the first year of experimentation at 25 days after transplanting*

***S. diameter*** *2(25 DAT) means the stem diameter of plant in the second year of experimentation at 25 days after transplanting*

3.1.2.3 Number of leaves

Table 3 shows the effect of treatments on the number of leaves of tomato plants over two years. Statistical analysis indicates that, overall, the treatments did not have a statistically significant effect on this parameter. However, significant effects were observed at 15 days after transplanting (DAT) during the first year and at 25 DAT in the second year of experimentation. Although no significant differences were noted globally, the application of 10 t/ha of organic matter promoted an increase in leaf number across all irrigation levels, unlike the 5 t/ha application, whose effects were less consistent. These findings suggest that applying 10 t/ha of organic matter, combined with supplementary irrigation, may enhance leaf number, even if this increase is not consistently statistically significant.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Treatments** | **Number of Leave1(15 DAT)** | **Number of Leave2(15 DAT)** | **Average** | **Number of Leave1(25 DAT)** | **Number of Leave2(25 DAT)** | **Average** |
| C10 + 100% | 9,82± 0,50ab | 6,40±0,21ab | 8,11±0,33 | 14,95± 1,01a | 10,60±0,36 | 12,78±0,59 |
| C5+ 100% | 8,37± 0,44b | 6,40±0,20ab | 7,39±0,27 | 11,42± 0,65b | 10,95±0,29 | 11,19±0,36 |
| CO + 100% | 9,02± 0,42ab | 6,23±0,21abc | 7,63±0,28 | 12,85± 0,92ab | 10,80±0,30 | 11,83±0,5 |
| C10+ 75% | 10,52± 0,58a | 6,55±0,22ab | 8,54±0,38 | 15,02± 0,94a | 10,78±0,27 | 12,87±0,54 |
| C5 + 75% | 9,77± 0,57ab | 6,30±0,22ab | 8,04±0,36 | 15,10± 1,36a | 10,18±0,37 | 12,64±0,76 |
| CO + 75% | 9,47± 0,47ab | 5,60±0,16c | 7,54±0,33 | 13,97± 1,01ab | 10,18±0,24 | 12,08±0,56 |
| C10 + 50% | 9,50± 0,59ab | 6,70±0,21a | 8,1±0,35 | 13,50± 1,24ab | 10,38±0,33 | 11,94±0,66 |
| C5 +50% | 9,12± 0,32ab | 5,90±0,24bc | 7,51±0,27 | 11,57± 0,64b | 10,15±0,29 | 10,86±0,36 |
| CO + 50% | 9,35± 0,35ab | 6,13±0,22abc | 7,74±0,27 | 12,72± 0,66ab | 10,23±0,33 | 11,48±0,4 |
| Probability | 0,14 | 0,014 | 0,205 | 0,03 | 0,437 | 0,09 |
| Signification | ns | \* |  | \* | ns | ns |

**Table 3. Effect of treatment on the number of leaves at 15 and 25 DAT during the first and the second year of experimentation**

*ns means no significant*

*\* means significant when P˂ 0,005*

*Number of Leave1 (15 DAT) means the Number of leaves in the first year of experimentation at 15 days after transplanting.*

*Number of Leave 2(15 DAT) means the Number of leaves in the second year of experimentation at 15 days after transplanting.*

*Number of Leave1 (25 DAT) means the Number of leaves in the first year of experimentation at 25 days after transplanting.*

*Number of Leave1 (25 DAT) means the Number of leaves in the second year of experimentation at 25 days after transplanting.*

3.1.3. Effect of supplementary irrigation dose and organic matter dose on fruit characteristics

*3.1.3.1. Dimensions of fruit*

Table 4 illustrates the effect of treatments on fruit height and diameter. Statistical analysis indicates that, overall, treatments did not have a significant impact on these two parameters. However, during the first year of experimentation, a significant influence of treatments on fruit height was observed. Additionally, although no statistically significant differences were noted globally, the application of organic matter appeared to reduce fruit height while increasing fruit diameter. These findings suggest that, under supplementary irrigation, the application of organic matter, while not having a statistically significant effect, may tend to slightly decrease fruit height and increase fruit diameter.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Treatment** | **Fruit length1** | **Fruit length2** | **Average** | **Fruit diameter1** | **Fruit diameter2** | **Average** |
| C10 + 100% | 33,92 | 56,9 | 56,38 | 30,71 | 55,98 | 55,41 |
| C5+ 100% | 29,16 | 50,34 | 50,14 | 25,73 | 54,62 | 54,34 |
| CO + 100% | 28,89 | 57,06 | 56,98 | 25,12 | 46,93 | 46,88 |
| C10+ 75% | 31,15 | 50,64 | 50,28 | 27,54 | 49,28 | 48,89 |
| C5 + 75% | 34,32 | 51,1 | 50,68 | 29,83 | 49,32 | 48,83 |
| CO + 75% | 30,66 | 51,87 | 51,21 | 27,31 | 49,07 | 48,4 |
| C10 + 50% | 34,17 | 50,67 | 50,36 | 30,42 | 48,27 | 47,93 |
| C5 +50% | 36,74 | 50,62 | 50,39 | 32,49 | 48,86 | 48,57 |
| CO + 50% | 41,79 | 51,06 | 50,97 | 31,98 | 49,21 | 49,03 |
| P | 0,02 | 0,698 | 0,68 | 0,23 | 0,471 | 0,47 |
| Significant | \* | ns | ns | ns | ns | ns |

**Table 4. Effect of treatment on fruit length and fruit diameter during the first and the second year of experimentation**

*ns means no significant*

*\* means significant when P˂ 0,05*

*Fruit length1 means fruit length in the first year of experimentation*

*Fruit length2 means fruit length in the second year of experimentation*

*Fruit diameter1 means the fruit diameter in the first year of experimentation*

*Fruit diameter2 means the fruit diameter in the second year of experimentation*

*3.1.3.3. Weight of fruit*

Table 5 highlights the effect of different treatments on fruit weight. Statistical analysis reveals that the treatments had a significant impact on this parameter, both globally and for each year. However, in the first year, the effect of the different treatments on fruit weight was quite mixed. In contrast, during the second year, within the D75 and D100% irrigation levels, the application of organic matter at rates of 10 and 5 t/ha led to an increase in fruit weight. Conversely, at the D50% irrigation level, the application of organic matter resulted in a decrease in fruit weight. Overall, the treatments produced relatively uniform fruit weights, except for the treatment C0+D100%, which resulted in a 9% reduction in fruit weight compared to the average of the other treatments. These findings emphasize that, under supplementary irrigation, the application of organic matter is indispensable for achieving higher fruit weights. However, when water requirements are reduced by half, the application of organic matter could be detrimental to fruit weight.

**Table 5. Effect of treatment on fruit weight during the first and the second year of experimentation**

|  |  |  |  |
| --- | --- | --- | --- |
| **Treatments** | **Weight of fruit1(g)** | **Weight of fruit2(g)** | **Average(g)** |
| C10 + 100% | 20,15± 1,26ab | 64,80±0,62a | 63,78±0,66a |
| C5+ 100% | 15,25± 1,14b | 64,91±1,04a | 64,42±1,05a |
| CO + 100% | 22,75± 7,84ab | 59,07±0,70b | 58,95±0,7b |
| C10+ 75% | 23,00± 2,38ab | 65,19±0,62a | 64,41±0,64a |
| C5 + 75% | 22,65± 2,18ab | 65,47±0,61a | 64,38±0,65a |
| CO + 75% | 17,04± 1,51b | 64,14±0,66a | 62,61±0,71a |
| C10 + 50% | 19,50± 1,93ab | 64,08±0,80a | 63,23±0,82a |
| C5 +50% | 27,88± 3,47a | 64,94±0,66a | 64,21±0,67a |
| CO + 50% | 28,60± 5,16a | 65,56±0,72a | 65,15±0,73a |
| P | 0,01 | 0,001 | 0 |
| Significant | \*\* | \*\* | \*\* |

*\* means significant when P˂ 0,05*

*\*\*means significant when P˂ 0,01*

*weight of fruit1(g) means weight of fruit in the first year of experimentation*

*Weight of fruit2(g) means weight of fruit in the second year of experimentation*

3.1.4. Effect of supplementary irrigation dose and organic matter dose on yield component

*3.1.4.1. Effect of supplementary irrigation dose and organic matter dose on yield*

Table 6 shows the effects of various treatments on tomato yield over two years. Statistical analysis indicates that the treatments did not significantly influence yield. However, the best yields were obtained with the C0+75% treatment. In addition, the application of organic matter at 5 and 10 t/ha increased yield, except at the D50% irrigation level, where the addition of 5 t/ha of organic matter resulted in a decrease in yield. Moreover, during the first year of experimentation, the application of organic matter at both 5 and 10 t/ha led to a reduction in tomato yield at the D50% irrigation level. These findings highlight that, although the addition of organic matter generally promotes higher yields, it becomes ineffective when water availability is reduced by half, leading to a decline in yields.

|  |  |  |  |
| --- | --- | --- | --- |
| Treatments | Yield(t/ha)1 | Yield(t/ha)2 | Average |
| C10 + 100% | 19,3± 3,35ab | 31,65±4,5 | 30,24±4,02 |
| C5+ 100% | 20,3± 2,77ab | 30,89±2,17 | 30,38±2,08 |
| CO + 100% | 15,1± 1,42b | 26,2±1,93 | 25,72±1,87 |
| C10+ 75% | 27,9± 5,52ab | 30,81±2,01 | 30,58±1,89 |
| C5 + 75% | 38,6± 9,95a | 31,1±2,01 | 31,17±1,97 |
| CO + 75% | 21,2± 3,69ab | 29,26±1,88 | 28,87±1,79 |
| C10 + 50% | 19,4± 5,58ab | 28,96±2,33 | 28,43±2,21 |
| C5 +50% | 22,7± 6,39ab | 25,14±1,98 | 24,74±1,87 |
| CO + 50% | 23,8± 7,34ab | 26,98±1,92 | 26,76±1,85 |
| Probability | 0,33 | 0,45 | 0,21 |
| Signification | ns | ns | ns |

**Table 6. Effect of Treatment on yield during the first and the Second year of Experimentation**

*Ns means no significance.*

*Yield(t/ha)1 means the yield in the first year of experimentation*

*Yield(t/ha) 2 means the yield in the second year of experimentation*

*3.1.4.1.* *Effect of supplementary irrigation dose and organic matter dose on water use efficiency (WUE)*

The effect of supplementary irrigation dose and organic matter dose on WUE is summarized in Table 7. Statistical analysis reveals a significant impact of the treatments on us. Although the addition of organic matter did not show a statistically significant effect at every irrigation level, it improved water use productivity at the d100 and d75 irrigation levels. Conversely, at the D50 irrigation level, the application of 5 t/ha of organic matter resulted in a decrease in WUE , while the application of 10 t/ha enhanced organic matter accumulation comparative with C0+ D50%. Consequently, the C10 + D50 treatment provided the highest WUE. Furthermore, during the first year of experimentation, the use of organic matter generally led to a reduction of WUE across all irrigation levels. This reduction was particularly pronounced at the D50 level, where the application of 10 t/ha of organic matter caused a significant 79% decline. These findings suggest that, within the context of supplemental irrigation, the application of organic matter can enhance WUE however, its effectiveness is highly dependent on the irrigation level.

**Table 7. Effect of treatment on water use efficiency (WUE)**

|  |  |  |  |
| --- | --- | --- | --- |
| Treatment | WUE1(Kg/m3) | WUE2(Kg/m3) | Average |
| C10 + 100% | 2,53 ± 0,43bc | 3,70±0,52c | 3,57±0,47a |
| C5+ 100% | 5,46 ± 1,08abc | 3,60±0,25c | 3,57±0,24ab |
| CO + 100% | 8,68 ± 2,35ab | 3,06±0,22c | 3,02±0,22ab |
| C10+ 75% | 2 ,65 ± 0,36bc | 5,40±0,35b | 5,39±0,33b |
| C5 + 75% | 7,57 ± 1,95abc | 5,45±0,35b | 5,56±0,36b |
| CO + 75% | 8,24 ± 2,31ab | 5,14±0,33b | 5,11±0,32ab |
| C10 + 50% | 1,97 ± 0,17bc | 10,16±0,81a | 10,05±0,77c |
| C5 +50% | 4,16 ± 0,72abc | 8,82±0,69a | 8,77±0,66c |
| CO + 50% | 9,54 ± 2,81a | 9,46±0,67a | 9,47±0,65c |
| P | 0 | 0,001 | 0.000 |

**3.2. Discussion**

In the context of supplementary irrigation, the effectiveness of organic matter application on agronomic performance remains a complex and not systematically conclusive issue. Regarding plant height, often used as a key indicator of vegetative vigor, the results show no significant variation throughout the growth phases of tomato plants, consistently across the two years of experimentation. Variability in irrigation doses and organic matter application tended to homogenize plant height. Similar results were reported by [19]who observed comparable plant height growth in tomatoes despite the application of compost at rates of 30, 40, 50, and 60 t/ha. Conversely [20]observed greater tomato height growth following the application of organic fertilizer. However, it should be noted that these organic fertilizers consist of a complex mixture of elements, including organic matter, nutrients, nitrogen-fixing and nitrifying bacteria, vitamins, and amino acids, which accelerate plant metabolism and growth. Organic matter had a fortifying effect on mineral elements, making them more available to plants. Furthermore, studies by [21] highlighted the positive correlation between nitrogen application and plant height growth. In this study, our results may be explained by the fact that the organic matter was insufficiently mineralized to release nitrate nitrogen, as suggested by [22]Additionally, nitrogen in compost is provided in organic form, requiring transformation into mineral nitrogen for optimal plant assimilation [23]. Concerning collar diameter, the results revealed that, overall, under supplementary irrigation conditions, growth phases and the application of 10 t/ha of organic matter significantly influenced this parameter. This finding extends to the number of leaves, although the observed increase in leaf number was not statistically significant. Specifically, results show that in the first year, the effects of treatments on these two parameters were significant only at 25 days after transplanting (DAT). Conversely, at 15 DAT, these parameters were not significantly affected by treatments. Several studies have demonstrated that sufficient moisture combined with organic matter application promotes an increase in leaf number and collar diameter. The results of this study may be attributed to uniform daily irrigation of all plots with 15,000 mm of water per plot during the [0–15 DAT] period in the first year to ensure the vigor of young transplanted plants. Furthermore, during this period, the applied compost might not have reached an advanced mineralization stage. The application of varying irrigation doses, initiated at 16 DAT, introduced variability that likely influenced collar diameter and leaf number significantly, despite the compost not completing its mineralization process. However, in the second year, the effects of treatments on these parameters were significant at 15 DAT, whereas at 25 DAT, only collar diameter was significantly affected. This difference might be due to second-year rainfall and minerals from the decomposition of compost applied in the first year, which could have significantly influenced collar diameter and leaf number during the [0–15 DAT] period. This effect persisted after applying different irrigation doses up to 25 DAT for collar diameter. However, for leaf number, treatments had no significant effect at 25 DAT in the second year, possibly due to plants reaching a maximum leaf number before 25 DAT under favorable conditions. The results further reveal that compost application at 10 t/ha systematically increased collar diameter and leaf number, although this increase was not always statistically significant. Conversely, a compost dose of 5 t/ha resulted in less consistent increases. These findings suggest that applying organic matter at 10 t/ha enhances water efficiency on plant growth parameters. Studies by [24] showed significantly more pronounced results, demonstrating that higher organic matter doses of 25 and 50 t/ha under all irrigation regimes notably favored plant height growth and increased leaf numbers across nearly all growth stages. Similarly, [25]reported that 100% soil-incorporated compost led to greater aerial growth compared to 25% and 50% rates. Thus, our findings indicate that while organic matter plays a critical role in crop growth, its optimal efficacy appears to be at a dose of 10 t/ha, with lower doses potentially constraining crop development.

Regarding fruit dimensions, the results indicate that, under supplementary irrigation, the effect of organic matter on fruit size depends on the irrigation dose. While organic matter application did not significantly impact fruit dimensions, its incorporation under D100 and D75 irrigation levels resulted in reduced fruit height and increased diameter. Conversely, under D50 irrigation, organic matter application reduced both fruit length and diameter. A similar trend was observed for fruit weight and yield. Under supplementary irrigation, organic matter application appears essential for achieving favorable fruit dimensions. However, when water availability is reduced by half, organic matter application may be detrimental. This observation could be attributed to inadequate water supplies preventing root systems from effectively absorbing necessary mineral elements. Water deficits negatively impact plant physiological processes, including nutrient uptake, photosynthesis, and overall growth, despite adequate mineral fertilization [26]. Studies by [15] similarly affirmed that organic matter's effectiveness is limited under severe water stress. For D100 and D75 doses, the results align with [20] who reported significantly larger fruits following organic fertilizer application. Likewise,[27] noted doubled maize length and weight after compost incorporation. Studies by[14] [28][29] also reported improved yields following compost application. Organic matter contributes essential nutrients, enhances nutrient uptake efficiency, and creates optimal soil moisture conditions. [30]demonstrated that the high adsorption capacity and porous characteristics of biochar allow water and nitrogen to remain longer in the soil, promoting water-nitrogen synergy and enhancing yields. These results underscore the crucial importance of organic matter application in enhancing both fruit dimensions and yields. They also suggest that the beneficial effects of organic matter may be limited under severe water stress conditions.

Regarding WUE, the results indicate a linear relationship between reduced water requirements and irrigation water productivity. Specifically, a reduction of 25% and 50% in water requirements led to respective increases in WUE of 58% and 178%. Several authors have highlighted this linear relationship between reduced water requirements and increased WUE [31], [32] However, this relationship is not consistent when considering organic matter application. Generally, compost application by 10t/ha and 5t/ha increased WUE under the D100 and D75 irrigation regimes. Conversely, it is observed that within the D50% irrigation dose, the application of compost at 10 t/ha led to an increase in WUE, whereas an application of compost at 5 t/ha resulted in a decrease in WUE. Overall, the combination C10+50% (10.05 kg/m³) resulted in the highest WUE, followed by C0+50% (9.47 kg/m³) and C5+50% (8.77 kg/m³). These results can be attributed to the ability of compost to enhance the soil’s water retention capacity and stabilize nutrients by reducing leaching[33]. However, when water availability is reduced by half, the water retained with a compost application of 5 t/ha is insufficient to meet both the plant’s water and nutrient requirements. Consequently, the lowest yields were observed with the C5+50% treatment (see table 6).

These findings reaffirm the critical role of organic matter application in stimulating crop growth, increasing fruit size, improving yields, and optimizing water productivity. However, they also highlight that, under severe water stress conditions, organic matter application can become a limiting factor for tomato production and water use efficiency. Thus, in the context of supplemental irrigation, the management of organic matter should be adjusted based on the severity and frequency of drought episodes and the availability of water to offset periodic water deficits.

4. Conclusion

In this study, under supplemental irrigation conditions, treatments combining different irrigation levels with varying doses of compost were compared to evaluate the effect of compost application on tomato productivity and water use efficiency. The results showed that applying compost at a rate of 10 t/ha significantly improves tomato growth parameters. Moreover, the findings suggest that when the water requirements of tomatoes are fully met or reduced by 25% (D100 and D75), compost application at 5 or 10 t/ha enhances fruit size, yield, and water productivity. However, when water availability is reduced by 50% (D50), compost application by 5t/ha may adversely affect tomato production and WUE. Therefore, the results recommend applying 5 t/ha of compost in combination with irrigation covering 75% of the plant’s water needs under supplemental irrigation conditions. Conversely, in scenarios where recurrent drought and limited or insufficient supplemental water are anticipated, the findings suggest applying 10t/ha of compost to avoid yield losses.

These recommendations can be adapted to dry climates and arid soils, particularly in regions where winter drought episodes constrain agricultural production.

DISCLAIMER (ARTIFICIAL INTELLIGENCE) Author(s) hereby declare that no generative AI technologies such as large language models (ChatGPT, copilot, etc) and text-to-image generators have been used during the writing or editing of manuscripts.

References

[1] R . Bilton , M.Gerber.,P. Grolier, C. Leoni, C., 2001. The White Book on Antioxidants in

Tomatoes and Tomato Products and Their Health Benefits: Role and Control of

Antioxidants in the Tomato Processing Industry.F. ( 2nd edd.). CMITI Sarl as a supplement to Tomato News

[2] S. Savić, R. Stikić, B. V. Radović, B. Bogičević, Z. Jovanović, and V. H. T. Šukalović.(2008). Comparative effects of regulated deficit irrigation (RDI) and partial root-zone drying (PRD) on growth and cell wall peroxidase activity in tomato fruits. Sci Hortic, 117(1),15–20, doi: 10.1016/j.scienta.2008.03.009.

[3] D. Son, I. Somda, A. Legrève, and B. Schiffers.(2017).Pratiques phytosanitaires et risques liés à l’usage des pesticides en culture de tomates au Burkina Faso.

[4] S. Assonsi. (2020). Market gardening around the industrial zone of kossodo a ouagadougou: practices, marketing channels and risks to the health of city dwellers revue espace, territoires, sociétés et santé, 3 (5), 67-78

[5] H. Zhang, Y. Xiong, G. Huang, X. Xu, and Q. Huang. (2017). Effects of water stress on processing tomatoes yield, quality and water use efficiency with plastic mulched drip irrigation in sandy soil of the Hetao Irrigation District. Agric Water Manag, 179, 205–214, doi: 10.1016/j.agwat.2016.07.022.

[6] Cristina Patanè, Simona Tringali and Orazio Sortino (2011). Effects of deficit irrigation on biomass, yield, water productivity and fruit quality of processing tomato under semi-arid Mediterranean climate conditions. Scientia Horticulturae,129 (4), 590-596.

[7] F. Favati, S. Lovelli, F. Galgano, V. Miccolis, T. Di Tommaso, and V. Candido. (2009). Processing tomato quality as affected by irrigation scheduling. Sci Hortic, 122( 4) , 562–571. doi: 10.1016/j.scienta.2009.06.026.

[8] L. U. Pulupol, M. Hossein Behboudian, and K. J. Fisher. (1996). Growth, Yield, and Postharvest Attributes of Glasshouse Tomatoes Produced under Deficit Irrigation. HORTSCIENCE, 31(6), 926-929,

[9] Costa, J.M., Ortuño, M.F. and Chaves, M.M. (2007) Deficit Irrigation as a Strategy to Save Water: Physiology and Potential Application to Horticulture. Journal of Integrative Plant Biology, 49, 1421-1434. Doi: http://dx.doi.org/10.1111/j.1672-9072.2007.00556.x

[10] Inmaculada Lahoz, Ana Pérez-de-Castro, Mercedes Valcárcel, Juan Ignacio Macua, Joaquim Beltrán, Salvador Roselló et al. (2016). Effect of water deficit on the agronomical performance and quality of processing tomato. Scientia Horticulturae, 200, 55-65 DOI: https://doi.org/10.1016/j.scienta.2015.12.05

[11] B. A. E. Van De Wal, H. A. L. Van De Put, J. Hanssens, and K. Steppe. (2017). Modelling the effects of osmotic stress on tomato fruit development. Acta Horticulturae, International Society for Horticultural Science. 201–206. doi: 10.17660/ActaHortic.2017.1154.26.

[12] You Wu, Wei Si , Shicheng Yan , Lifeng Wud, Wenju Zhao, Jiale Zhang, Fucang Zhang and Junliang Fan*.*(2023). Water consumption, soil nitrate-nitrogen residue and fruit yield of drip-irrigated greenhouse tomato under various irrigation levels and fertilization practices. Agric Water Manag, 277 Doi: 10.1016/j.agwat.2022.108092.

[13] Bruno Glaser, Johannes Lehmann, Christoph Steiner, Thomas Nehls, Muhammad Yousaf and Wolfgang Zech. (2002). Potential of Pyrolyzed Organic Matter in Soil Amelioration. Biology and fertility of soils. 12th ISCO conference, 421-427

[14] S. S. Akhtar, G. Li, M. N. Andersen, and F. Liu. (2014). Biochar enhances yield and quality of tomato under reduced irrigation. Agric Water Manag, 138, 37–44, doi: 10.1016/j.agwat.2014.02.016.

[15] M. Ekinci, S. Ors, U. Sahin, E. Yildirim, and A. Dursun. (2015). Responses to the Irrigation Water Amount of Spinach Supplemented with Organic Amendment in Greenhouse Conditions, Commun Soil Sci Plant Anal,46(3), 327–342, doi: 10.1080/00103624.2014.980827.

[16] E. Gavili, A. A. Moosavi and F. Moradi Choghamarani.(2018). Cattle manure biocty -40 har potential for ameliorating soil physical characteristics and spinach response under drought. Arch Agron Soil Sci, 64(12) 1714–1727, doi: 10.1080/03650340.2018.1453925.

[17] S. M. Farahani and M. R. Chaichi, (2013). Whole Forage Barley Crop Quality as Affected by Different Deficit Irrigation and Fertilizing. Systems.*Commun* Soil Sci Plant Anal, 44(20),2961–2973. doi: 10.1080/00103624.2013.829848.

[18] Geerts, S. and Raes, D. (2009) Deficit Irrigation as an On-Farm Strategy to Maximize Crop Water Productivity in Dry Areas. Agriultural Water Management, 96, 1275-1284.  
http://dx.doi.org/10.1016/j.agwat.2009.04.009.

[19] M.A.Kitabala, U.J. Tshala, M. A. Kalenda, I. M. Tshijika, K. M. Mufind. (2016). Effets de différentes doses de compost sur la production et la rentabilité de la tomate (Lycopersicon esculentum Mill) dans la ville de Kolwezi. Province du Lualaba (RD Congo). Journal of Applied Biosciences, 102, 9669-9679.

[20] A. Coulibaly, J. Ouédraogo, S. Roseline NACRO and I. Serme. (2022). Effets des fertilisants organiques sur la production de la tomate et les paramètres chimiques du sol au Centre Nord du Burkina Faso. Afrique science, 21(4),10 - 27

[21] Satognon, F., Owido, S.F.O. and Lelei, J.J. (2021). Effects of supplemental irrigation on yield, water use efficiency and nitrogen use efficiency of potato grown in mollic Andosols. Environ Syst Res, **10** (38), 2193-2697 https://doi.org/10.1186/s40068-021-00242-4

[22] Bacyé, B. (1993) Influence des systèmes de culture sur l’évolution du statut organique et minéral des sols ferrugineux et hydromorphes en zone soudano-sahélienne. (Province du Yatenga, Burkina Faso). Thèse de doctorat en sciences, Université de Droit, d’Economie et des Sciences d’Aix-Marseille III, France.

[23] J. G. Cobo, Edmundo Barrios Donald C. L. Kass and Richard Thomas. (2022). Nitrogen mineralization and crop uptake from surface-applied leaves of green manure species on a tropical volcanic-ash soil Biol Fertil Soils. 36,87–92 DOI 10.1007/s00374-002-0496-y

[24] G. H. D. Agbna, S. Dongli, L. Zhipeng, N. A. Elshaikh, S. Guangcheng and L. C. Timm. (2017). Effects of deficit irrigation and biochar addition on the growth, yield, and quality of tomato. Sci Hortic, 222, 90–101, doi: 10.1016/j.scienta.2017.05.004.

[25] B. Mouria, A. O. Touhami and A. Douira. (2010). Valorisation agronomique du compost et de ses extraits sur la culture de la tomate [Online]. Available: <https://www.researchgate.net/publication/312192203>

[26] B Sarkar, Y Varalaxmi, M Vanaja, N RaviKumar, M Prabhakar, SK Yadav et al. (2023). Mapping of QTLs for morphophysiological and yield traits under water-deficit stress and well-watered conditions in maize. Front Plant Sci, 14, 1124619. doi: 10.3389/fpls.2023.1124619..

[27] L. Mrabet, D. Belghyti, A. Loukili, and B. Attarassi, (2011). Étude de l’effet du compost des déchets ménagers sur l’amélioration du rendement de Maïs et de la Laitue. Afrique SCIENCE 07(2), 74-84

[28] O. T. Faloye, M. O. Alatise, A. E. Ajayi, and B. S. Ewulo, (2019). Effects of biochar and inorganic fertiliser applications on growth, yield and water use efficiency of maize under deficit irrigation. Agric WaterManag, 217,165–178, doi: 10.1016/j.agwat.2019.02.044.

[29] Z. Abideen, H. W. Koyro, B. Huchzermeyer, R. Ansari, F. Zulfiqar,B. Gul.(2020). Ameliorating effects of biochar on photosynthetic efficiency and antioxidant defence of Phragmites karka under drought stress. Plant Biol,22(2), 259–266, doi: 10.1111/plb.13054.

[30] P. Zhang, J.Liu, M. Wang; H. Zhang, N. Yang, J. Ma et al. (2024). Effect of irrigation and fertilization with biochar on the growth, Yiekd and water/nitrogene use of maize on the Guanzhong Plain, China.Agric Water Manag, 295,108786

[31] J. Lu, G. Shao, J. Cui, X. Wang, L. Keabetswe. (2019). Yield, fruit quality and water use efficiency of tomato for processing under regulated deficit irrigation: A meta-analysis. Agric Water Manag, 22, 301–312, Aug. 2019, doi: 10.1016/j.agwat.2019.06.008.

[32] J. Xu *et al.*, “Effect of Regulated Deficit Irrigation on the Growth, Yield, and Irrigation Water Productivity of Processing Tomatoes under Drip Irrigation and Mulching,” *Agronomy*, 13(12),2862, doi: 10.3390/agronomy13122862.

[33] Paulin, R. and O’Malley, P.J. (2008) Compost Production and Use in Horticulture. Bulletin/Western Australia, Department of Agriculture and Food, South Perth.  
http://archive.agric.wa.gov.au/objtwr/imported\_assets/content/hort/compost\_bulletin08.pdf.