**Harnessing the Potential of Napier Grass (*Pennisetum purpureum*) for Sustainable Biofuel Production**

**Abstract**

Napier grass (*Pennisetum purpureum*) is an energy-rich C4 perennial grass that has potential as a biofuel feedstock for sustainable growth. It originally comes from Africa but can cultivated in tropical and subtropical regions, producing 25–35 oven-dry tons per hectare per annum, much greater than other energy grasses. Its low-input growth requirements, weeding capacity, and intercropping system compatibility render it yet more desirable as a renewable power source. Napier grass is most useful to produce biofuel since it yields bioethanol and biogas with minimal interference in the food supply. Its cellular content, with high carbohydrate and lignocellulosic compound contents, provides effective biochemical conversion with minimum wastage. In addition, the grass shows resistance against drought, allowing it to grow well in water-scarce regions. This review examines the botanical traits, growth requirements, and biofuel production capacity of Napier grass, noting its strengths and potential in renewable energy projects. By overcoming challenges like genetic variability, disease tolerance, and water efficiency, Napier grass can be central to the shift toward sustainable bioenergy systems.

**Keywords:** Napier grass, biofuel, biomass, bioethanol, biogas, carbon sequestration, renewable energy, sustainable agriculture, lignocellulosic biomass, biochar.

1. **Introduction**

Napier grass (*Pennisetum purpureum*) is a high-yielding C4 perennial grass that has excellent prospects as a biofuel feedstock due to the fact that it is versatile, low-cost, and has rapid growth (Chiluwal *et al.,* 2019). Native to Africa alone, it flourishes in the tropical and subtropical areas and produces 25–35 oven-dry tons per hectare per annum equivalent to some 100 barrels of oil energy per hectare. With a harvest of six or more crops per annum, it outcompetes other energy grasses such as miscanthus and switchgrass in biomass production (Prapinagsorn *et al.,* 2017). Napier grass is a low-input crop, weeds-suppressing, and productive in poor soils and thus a low-input energy crop (Hattori & Morita, 2015). It can further be intercropped with oil palm, making use of 26.63% of otherwise vacant plantation land and increasing biomass yield. Compared to switchgrass that yields about 23 Mg/ha, Napier grass yields up to 50 Mg/ha, hence avoiding soil erosion and nutrient loss by runoff (Amaducci *et al.,* 2017). As a second-generation biofuel crop, Napier grass does not compete with food crops, unlike first-generation biofuels (Pensri *et al.,* 2016; Negawo *et al.,* 2017). Its biofuels, biodiesel and bioethanol, fight climate change by reducing the use of fossil fuels, which are among the major carbon emission sources (Azeke *et al.,* 2019). Its production also acts as an economic driver through the creation of employment for bioenergy specialists   
Napier grass is also suitable for biogas production with its methane content reaching up to 63.50%. According to research, NaOH-pretreated biomass yields more biogas than raw samples (Dussadee *et al.,* 2017). These characteristics make Napier grass an ideal and renewable source for future bioenergy.

1. **Botanical and Agronomic Characteristics of Napier Grass**
   1. **Taxonomy and Morphology**


Napier grass belongs to Poaceae family and is a notable C4 perennial grass growing up to a height of 7.5 meters. Its large root system can grow as deep as 4.5 meters, rendering it extremely drought-tolerant and potentially a great asset for carbon sequestration (Yang *et al.,* 2019). The grass has a sturdy stem close to the base, roughly 3 cm in diameter, and has long blades that extend up to 120 cm long and 5 cm wide.  
Napier grass has excellent tillering that makes it produce a wide leaf area and have good interception of solar radiation. It possesses a long canopy and preserves a high level of photosynthesis, exhibiting maximum radiation use efficiency among other C4 plants. A single plant of each variety can yield between 35 and 100 tillers, depending on the time of year (Amin *et al.,* 2016). The leaf/stem ratio of Napier grass varies from 0.57 to 1.63 (Halim *et al.,* 2013) and usually includes a higher proportion of leaves versus stems in its dwarf varieties. Though it has its optimal development under full sun (Anderson *et al.,* 2008), Napier grass is also found to tolerate shade. Generally, it has all the necessary traits for high productivity such as intensive tillering, a high leaf area, and an erect canopy, which make it more productive than maize.

* 1. **Growth Conditions and High Biomass Yield**

When cultivated in tropical and subtropical climates, grasses utilizing the C4 photosynthetic pathway are believed to possess a competitive edge over C3 grass species (Taylor *et al.,* 2011). Napier grass, a C4 species, is particularly notable for its ability to decrease shoot dry matter while maximizing carbon assimilation during periods of water scarcity, rendering it an advantageous forage crop in regions prone to intermittent droughts (Cardoso *et al.,* 2015). Its characteristics, which encompass high dry matter production, ease of establishment and regeneration, persistence, and improved water use efficiency, establish Napier grass as the preferred forage in Eastern and Central Africa, where smallholder dairy farmers and pastoralists contend with sporadic droughts and limited irrigation resources. Under water stress conditions, Napier grass exhibits morphological adaptations such as leaf rolling, reduced stomatal conductance, and enhanced water use efficiency. As a perennial crop, it is anticipated that Napier grass will encounter fluctuations in rainfall, leading to water stress at various times throughout the year; reports indicate that cultivars may experience a yield potential reduction of up to 20% when subjected to water-deficient conditions compared to a control environment (Purbajanti *et al.,* 2012). Consequently, the development of cultivars capable of enduring and producing during brief drought periods is deemed beneficial for regions lacking irrigation, especially in light of the anticipated impacts of climate change on an increasing number of areas. The successful cultivation of forage is contingent upon the ability to mitigate the trade-off between dry matter production and yield potential under stress conditions such as drought. Research has shown that biomass yield loss in Napier grass is less pronounced than that observed in Guinea grass when subjected to water stress. Napier grass has historically received limited research investment, resulting in minimal progress in its breeding compared to other forage species (Mwendia *et al.,* 2014). Furthermore, the absence of genomic tools specific to Napier grass has hindered breeding efforts but if a suitable genomic toolbox is developed and the physiological responses to water stress are thoroughly understood, it is anticipated that cultivars capable of withstanding intermittent drought can be created in the near future. Currently, the water use efficiency of various accessions from the ILRI (International Livestock Research Institute) forage genebank is being assessed in both irrigated and non-irrigated conditions. This evaluation will enhance our understanding of their drought response mechanisms and lay the groundwork for the development of more drought-tolerant Napier grass cultivars.

**Figure 1:** Biorefinery Process of Elephant Grass Biomass

1. **Potential of Napier Grass in Biofuel Production**

Napier grass (*Pennisetum purpureum*) is a fast-growing, high-biomass grass species that shows great promise as a feedstock for biofuel production. Due to its high yield and suitability for various conversion processes, it is increasingly being considered as an alternative source of renewable energy.

* 1. **Composition and Energy Content**

Bioethanol is a renewable biofuel from biomass and crop residues, which makes it an environmentally friendly fuel with clean exhausts. Thailand, with richness in biodiversity and diversity of energy crops—mostly grasses—has an excellent potential for the production of bioethanol. Unlike first-generation ethanol, which uses sugar crops, second-generation bioethanol targets lignocellulosic feedstocks like energy crops and crop wastes. This method helps address food safety concerns by utilizing biomass that is non-food (Restiawaty *et al.,* 2020; Sanford *et al.,* 2017). Napier grass (*Pennisetum purpureum*) is commonly cultivated as animal fodder and is also a highly likely candidate for making bioethanol.

It is a high-yielding, fast-growing crop, and it is possible to harvest it year-round, thus a stable source of bioenergy. Its nutrient content is 30.9% carbohydrates, 27% proteins, 14.8% lipids, 18.2% total ash, and 9.1% fiber (dry weight) (Sawasdee & Pisutpaisal, 2014). Napier grass is highly carbohydrate-containing grass and serves as a suitable precursor for the bioconversion of ethanol. In composition, it has about 45%–50% cellulose, 30%–32% hemicellulose, and 18%–22% lignin (Reddy *et al.,* 2014; Kommula *et al.,* 2013). Different studies have conducted various Napier grass conversion processes to bioethanol examined the effect of some pretreatment and fermentation processes, using *Saccharomyces cerevisiae* and *Scheffersomyces shehatae*, a xylose-fermenting yeast (Kongkeitkajorn *et al.,* 2020).

Their results indicated that NaOH pretreatment of Napier grass followed by individual hydrolysis and fermentation (SHF) yielded the maximum concentration of ethanol (44.7 g/L). It was also demonstrated that simultaneous saccharification and fermentation (SSF) of *S. cerevisiae* and cellulase (CTec2) after alkaline pretreatment produced 0.143 g of ethanol per gram of raw material (Tsai *et al.,* 2018). Hydrolysis (the chemical breakdown of a compound due to reaction with water) and fermentation (substance breaks down into a simpler substance) are the most important steps in the production of bioethanol. Hydrolysis methods include enzymatic, acidic, and alkaline processes (Kusmiyati *et al.,* 2016). In conventional SHF, cellulose is hydrolyzed into fermentable sugars before the process of ethanol fermentation.

This technique, however, consumes a lot of energy and entails several steps in processing (Cotana *et al.,* 2015). SSF, on the other hand, merges both procedures into one, reducing investment and operational costs. Research suggests that SSF outperforms SHF by yielding higher ethanol production and reducing enzyme degradation (Dahnum *et al.,* 2015; Xu *et al.,* 2015). This advantage is attributed to lower levels of glucanase and cellobiohydrolase in SSF, which enhances efficiency. In SSF, enzymes remain more stable due to reduced sugar accumulation, which minimises feedback inhibition and degradation, leading to improved ethanol yield without necessarily lowering enzyme dosage.

Additionally, experiments using acid mine drainage for pretreatment have shown ethanol yields of 14.43 g/L for SHF and 14.83 g/L for SSF. Enzymes also play a crucial role in converting lignocellulose into fermentable sugars (Banka *et al.,* 2015; Loaces *et al.,* 2017; Burman *et al.,* 2019). In addition, fungal enzymes, especially those from *Trichoderma reesei* mutant strains, are widely applied in cellulose degradation (Gusakov *et al.,* 2011). While yeast strains such as *S. cerevisiae*, *Scheffersomyces stipitis*, and *Schizosaccharomyces pombe* are effectively used in fermenting sugars to ethanol (Ariyanti & Hadiyanto, 2013). In reality, whole-cell fermentation with microorganisms is a less expensive method than commercial enzymes. In general, Napier grass is a potential feedstock for the production of bioethanol because it is readily available, rich in carbohydrates, and easy to use with many different fermentation methods. As techniques in pretreatment and fermentation continue to be improved, this energy crop will become a valuable addition to sustainable biofuel development (Azhar *et al.,* 2017).

**Table 1:** Composition and Energy Content of Napier Grass

|  |  |  |  |
| --- | --- | --- | --- |
| **Component** | **Role in Biofuel Production** | **Challenges** | **Solutions** |
| Cellulose | Main carbohydrate; hydrolyzed into fermentable sugars for bioethanol production. | Structural complexity limits accessibility. | Pretreatment methods improve enzymatic hydrolysis. |
| Hemicellulose | Converts into fermentable sugars more easily than cellulose. | Requires pretreatment for optimized conversion. | Acid/alkaline pretreatment enhances breakdown. |
| Lignin | Provides structural strength; can be used in thermochemical processes (pyrolysis/gasification). | Blocks enzymatic access to cellulose and hemicellulose. | Acid hydrolysis, steam explosion, and lignin-modifying enzymes. |

**3.2 Biofuel Production from Napier Grass**

Napier grass (*Pennisetum purpureum*) can be processed into biofuels, specifically ethanol, once it is fully matured. Almost all plant parts, such as leaves, stalks, and stems can be used for the production of bioethanol. Aside from ethanol, Napier grass can also be transformed into liquid and gaseous fuels. In liquid form, it can either be bioethanol or bio-oil. Yet, bioethanol is the better choice because bio-oil has a lower heating value (Treedet *et al.,* 2020). The production of bioethanol from Napier grass is a four-stage process lasting approximately 94 hours, involving pretreatment, hydrolysis, fermentation, and the final separation of ethanol.

**3.2.1 Pretreatment: Disintegration of the Biomass**

Pretreatment is the initial and most important step, encompassing processes such as harvesting, cleaning, drying, and grinding. Different pretreatment processes assist in breaking down the rigid structure of the biomass to facilitate easier extraction of fermentable sugars. These methods can be physical (such as grinding, milling, and extrusion at high temperatures) or chemical. Chemical treatments use substances like sulfuric acid, ammonia, sodium hydroxide, hydrogen peroxide, and acetic acid for processes like soaking, steam explosion, and oxidation (Campos *et al.,* 2019; Tsai *et al.,* 2018). The goal is to break down the crystalline cellulose structure, increase porosity, and make the biomass more accessible for further processing.

Before hydrolysis, analysis of proximate composition is performed to determine major parameters like moisture, lipid content, ash content, and crude protein. In some cases, the biomass is treated with different concentrations of sodium hydroxide, autoclaved at 121°C for an hour, and then neutralized and filtered.Another method includes thermal hydrolysis using steam or hot water to disrupt the biomass prior to drying for hydrolysis (Dussadee *et al.,* 2017).

**3.2.2 Hydrolysis: Converting Biomass into Sugars**

At this level, enzymes or acid hydrolysis are used in the depolymerization of the biomass into simple sugars. Enzyme mixtures with a maximum of 50 enzymes are also used to depolymerize different biomass components. Acid hydrolysis is another method, where dilute solution of sulfuric acid (0.5 M H₂SO₄) is added to the biomass and, after heating at 155°C for 30 minutes under steady stirring, is allowed to rest. The process can be controlled by the use of different concentrations of biomass (5g, 10g, 15g, or 20g) and adjusting pH to 5.0 through sodium hydroxide . In certain circumstances, cellulase enzymes from industries like iKnowzyme and Acid Cellulase are added to support further hydrolysis (Pensri *et al.,* 2016).

**3.2.3 Fermentation: Conversion of Sugars into Ethanol**

Fermentation is carried out in a medium rich in nutrients with dextrose sugar, yeast extract, and other basic nutrients. Such a medium is inoculated with *Saccharomyces cerevisiae* yeast and fermented at 35°C for 1 to 5 days before distillation at 78.3°C. Since *S. cerevisiae* does not tolerate heat, however, tropical areas have to use bioreactors fitted with cooling units, making it more expensive to produce. A substitute is *Kluyveromyces marxianus,* a heat-resistant yeast that minimizes cooling expenses but still ensures efficiency in ethanol production (Campos *et al.,* 2019).

**3.2.4 Comparing Biofuels: Solid, Liquid, and Gas**

Even though Napier grass can be converted to solid fuel, liquid and gaseous biofuels are desirable because they minimize greenhouse gas emissions. Most nations have put policies in place to promote the production of biofuels, bringing down their carbon footprints considerably (Treedet *et al.,* 2020). One method of using Napier grass as a gaseous fuel is through the production of biogas. Scientists investigated two major techniques: briquetting and anaerobic digestion . Briquetting is a process of pressing biomass into hard, combustible blocks that are ready to use as fuel. Anaerobic digestion, however, is a microbial process by which microorganisms digest the biomass under anaerobic conditions. This process involves four stages—hydrolysis, acidogenesis, acetogenesis, and methanogenesis—ending up with the production of methane-rich biogas (Divyabharathi & Venkatchalam, 2015).

**3.2.5 Pyrolysis: Production of Bio-Oil from Napier Grass**

Pyrolysis is a thermochemical process by which biomass is converted into bio-char (solid), bio-oil (liquid), and syngas (gas) in the absence of an oxygen environment (Mohammed *et al.,* 2015). Napier grass-based bio-oil has a blend of hydrocarbons and organic compounds. Though hydrocarbon content makes it flammable, organic acids and heterocyclic compounds cause its viscosity and tendency to polymerize . It has been established through studies that enhancing the rate of nitrogen flow to 20-30 mL/min and sustaining reaction temperatures at 450-600°C can yield optimum bio-oil (Mohammed *et al.,* 2017).

The increasing unavailability of fossil fuels has propelled the quest for alternative sources of energy. Furthermore, burning these non-renewable fuels to generate electricity emits greenhouse gases and toxic pollutants, which have serious implications for the environment and human health. Carbon emissions globally have been increasing at an alarming level. During the 1960s, fossil fuel combustion released an average of 3.1 GtC per year (gigatonnes of carbon, which is a unit of measurement representing one billion metric tonnes of carbon emissions released into the atmosphere**)** but between 2008 and 2017, the rate had almost reached three times that, at 9.4 GtC per year (Le Quere *et al.,* 2018). The continued consumption of fossil fuels as a source of energy, especially for industrial and transportation purposes, has been listed as one of the principal reasons for this crisis. This problem of a global nature has given rise to global cooperation, as seen in agreements like the Kyoto Protocol and the Paris Agreement, which aim to cap worldwide carbon emissions. Therefore, the majority of countries are now increasingly turning away from fossil fuels and embracing sustainable alternatives (Md Said *et al.,* 2019).

Minimizing dependence on scarce fossil fuels and exploring alternative renewable energy has now become a national priority. This commitment is evident in government policy such as the Five-Fuel Diversification Policy, which officially names renewable energy as the fifth fuel (Bujang *et al.,* 2016). A major strategy under this policy is encouraging the utilization of biomass, considering its prevalence in Malaysia. In order to extend the scope of biomass sources and contribute to greater diversification of energy resources, scientists have also been seeking newer renewable sources (Rebitanim *et al.,* 2013). Of these, Napier grass (NG) has received widespread attention owing to its high-energy crop potential. Native to Africa, Napier grass is not only very productive but also cheap to establish, and it gives around 40 tonnes per hectare per annum with multiple crops (Hlavsova *et al.,* 2014). Despite its potential, the use of Napier grass to generate green energy is an underdeveloped field. More than half of the research work on Napier grass has aimed to transform it into energy through the pyrolysis method of thermal decomposition (Suntivarakorn *et al.,* 2018). With its productivity and sustainability level, however, the discovery of more energy applications from Napier grass may significantly contribute to improving renewable energy initiative (Lee *et al.,* 2010).

**Table 2:** Napier Grass for Renewable Energy

|  |  |  |
| --- | --- | --- |
| **Aspect** | **Key Information** | **References** |
| Fossil Fuel Impact | Fossil fuel use has led to a sharp rise in carbon emissions, nearly tripling between 1960 and 2017. | Le Quere *et al.,* 2018 |
| Global Response | International agreements like the Kyoto Protocol and Paris Agreement aim to reduce carbon emissions. | Md Said *et al.,* 2019 |
| National Policies | Policies like the Five-Fuel Diversification Policy promote renewable energy as a key resource. | Bujang *et al.,* 2016 |
| Biomass Utilization | Malaysia is focusing on biomass due to its abundance, encouraging research into alternative sources. | Rebitanim *et al.,* 2013 |
| Napier Grass Potential | Highly productive and easy to cultivate, Napier grass yields about 40 tonnes per hectare annually. | Hlavsová *et al.,* 2014 |
| Current Research | Most studies on Napier grass focus on energy production through pyrolysis. | Suntivarakorn *et al.,* 2018 |
| Future Prospects | Further research may unlock new energy applications, enhancing its role in renewable energy initiatives. | Lee *et al.,* 2010 |

1. **Advantages of Napier Grass for Biofuel Production**

Napier grass (*Pennisetum purpureum*) is increasingly regarded as an ideal feedstock for biofuel production due to its numerous advantages. These advantages are not only related to its biomass yield and conversion efficiency but also its environmental benefits, such as carbon sequestration and soil conservation.

**Table 3:** Key benefits that make Napier grass a highly attractive option for biofuel production.

|  |  |  |
| --- | --- | --- |
| **Advantage** | **Description** | **Key Benefits** |
| High Productivity | Produces 150–200 tonnes of dry matter per hectare annually, surpassing other bioenergy crops like switchgrass and miscanthus. | Higher bioethanol and biogas yields; adaptable to diverse climates. |
| Low Input Requirements | Requires minimal fertilizers and pesticides; naturally pest-resistant. | Environmentally friendly and cost-effective. |
| Carbon Sequestration | Absorbs large amounts of CO₂, mitigating greenhouse gas emissions. | Offsets carbon emissions, contributing to climate change mitigation. |
| Soil Conservation | Dense root system prevents soil erosion and improves soil fertility. | Enhances land sustainability and reduces dependency on synthetic fertilizers. |

**Figure 2:** Key Advantages of Napier Grass for Biofuel Production

****

1. **Future Prospects and Recommendations**

Although there has been considerable progress in the cultivation and utilization of Napier grass (*Pennisetum purpureum)* as a biofuel crop, genetic diversity, disease resistance, and production methods remain issues. There are various opportunities to further enhance its performance to make it a suitable renewable energy crop to substitute for fossil fuels.  
  
**5.1 Enhancing Genetic Diversity for Biofuel Applications**

Napier grass has tremendous potential for biofuel production, especially as bioethanol and biogas. In order to maximize this potential, it is essential that the genetic diversity of available cultivars is improved. Although breeding programs have been launched, efforts are needed to incorporate contemporary molecular tools to hasten the creation of new varieties with enhanced biofuel yields (Faleiro *et al.,* 2016). Next-generation sequencing technologies and genomics as well as molecular genetics provide us with unprecedented promise for the detection of genetic attributes that can be targeted for pest resistance, higher biomass yield, and lignin content. Research today has the potential to target this variety through the process of genetic maps and sequence information, which could help in making cultivars better suited for the biofuel factor (Wanjala *et al.,* 2013).

**5.2 Overcoming Disease Constraints with Molecular Breeding**

Napier grass faces challenges from diseases such as stunt disease and head smut, which impact its production, especially in regions of Africa. Advances in molecular breeding can help in developing disease-resistant varieties by identifying resistance genes through genomic studies. As demonstrated in other crops, such as sugarcane, the introduction of genes conferring resistance to pathogens can significantly reduce the negative impacts of these diseases on yield and quality. For instance, varieties like 'Kakamega 1' and 'Kakamega 2' have been identified as resistant to smut disease, yet the mechanisms behind this resistance are not fully understood (Mwendia *et al.,* 2007). Future research can focus on identifying these resistance genes and introducing them into commercial cultivars. Moreover, gene editing technologies, such as CRISPR-Cas9, could be employed to enhance disease resistance in Napier grass and further improve its sustainability as a biofuel crop (Khan *et al.,* 2014).  
 **5.3 Improving Nutritional Quality for Livestock and Biofuel Production**

One more aspect of Napier grass to be considered is its nutritional value, particularly when it comes to its dual potential as an animal feed and a biofuel. The potential of Napier grass as a feedstock for producing biofuel as well as an improved pasture crop can be improved greatly by its digestibility improved through the elimination of its lignin content.Low-lignin cultivars have shown potential in increasing digestibility of forages, including those with brown midrib mutations in sorghum and maize (Sattler *et al.,* 2010). Plant breeders can increase the nutritional value of Napier grass for cattle and maximize its biomass for use as biofuels using the same method. Additionally, changing the structure of the lignin to make it digestible can increase the amount of bioethanol and other biofuels that can be obtained from Napier grass.

**5.4 Addressing Water Use Efficiency and Climate Adaptability**

Water use efficiency is another critical factor for the successful cultivation of Napier grass, especially in regions with limited rainfall or under the threat of climate change. Napier grass is generally considered a drought-tolerant species, but its water use efficiency could be further optimized to ensure better productivity in areas where rainfall is less than its optimal range of 750 mm per year. Research into genetic variations of Napier grass with enhanced water use efficiency is essential for its future success in marginal areas (Van De Wouw *et al.,* 1999). Integrating molecular breeding with environmental stress-resilience traits could allow for the development of 'climate-smart' Napier grass varieties that can withstand the challenges posed by climate change while contributing to sustainable bioenergy production.  
  
**5.5 Expanding Seed Propagation Techniques**

One other significant disadvantage of Napier grass is its reliance on vegetative propagation, limiting genetic diversity and disease transmission. Seed production practices are the driving force to produce Napier grass on a global scale. Hybrid varieties with controlled cross-pollination and improved seed propagation could maximize genetic diversity and productivity (Singh *et al.,* 2013). By increased seed production methods, Napier grass can be spread more widely, reducing the risk of disease transmission associated with vegetative propagation.

**Conclusion**

The study of Napier grass (*Pennisetum purpureum*) as a feedstock for biofuel indicates its massive potential to reduce the energy crisis in the world while conserving the environment. With high biomass production, low input needs, and resistance to different climatic stresses, Napier grass is a viable substitute for conventional fossil fuels. Its high production capacity for bioethanol and biogas makes it a central player in the renewable energy sector, especially where food security is the case. Napier grass benefits go beyond the potential of biomass yield. Its fibrous root system contributes to soil conservation and carbon sequestration, reversing the negative impacts of climate change. Moreover, the fact that grass can survive under conditions of drought indicates that it can be a successful crop for plantations in regions prone to drought, with the guarantee of a reliable source of bioenergy regardless of the weather conditions. While the world is grappling to manage the aftereffect of fossil fuel, farming of Napier grass provides the viable route toward greenhouse gas emission reduction and utilizing clean energy. But to harvest the maximum out of Napier grass in terms of biofuel production, many issues need to be addressed.  
Improving genetic diversity through new breeding techniques can lead to the development of cultivars with improved biomass yields, disease resistance, and nutritional value. The application of molecular breeding techniques can enable the selection of characteristics that enhance the grass's ability to adapt to climate change and increase its water use efficiency. Moreover, enhancing seed propagation techniques will reverse the limitations of vegetative propagation, offering greater genetic diversity and resistance to disease.   
In summary, the future of Napier grass as a biofuel crop is promising, provided that concerted efforts are made in enhancing its genetic and agronomic traits. By investing in research and development, policymakers and stakeholders can unlock the full potential of Napier grass, allowing a sustainable future in energy while promoting rural economies and environmental stewardship. As the world shifts towards renewable energy sources, Napier grass can be a door to sustainable production of biofuels, which will lead the way to a greener, more sustainable world.

Disclaimer (Artificial intelligence)

Option 1:

Author(s) hereby declare that NO generative AI technologies such as Large Language Models (ChatGPT, COPILOT, etc.) and text-to-image generators have been used during the writing or editing of this manuscript.

**References**

1. Amaducci, S., Facciotto, G., Bergante, S., Perego, A., Serra, P., Ferrarini, A., & Chimento, C. (2017). Biomass production and energy balance of herbaceous and woody crops on marginal soils in the Po Valley. *Gcb Bioenergy*, *9*(1), 31-45.
2. Adekunle, A., Orsat, V., & Raghavan, V. (2016). Lignocellulosic bioethanol: A review and design conceptualization study of production from cassava peels. *Renewable and Sustainable Energy Reviews*, *64*, 518-530.
3. Ariyanti, D., & Hadiyanto, H. (2013). Ethanol production from whey by Kluyveromyces marxianus in batch fermentation system: kinetics parameters estimation. *Bulletin of Chemical Reaction Engineering & Catalysis*, *7*(3), 179-184.
4. Azhar, S. H. M., Abdulla, R., Jambo, S. A., Marbawi, H., Gansau, J. A., Faik, A. A. M., & Rodrigues, K. F. (2017). Yeasts in sustainable bioethanol production: A review. *Biochemistry and biophysics reports*, *10*, 52-61.
5. Azeke, E. M., Eze, C. L., Ubong, I., & Kuroshi, L. (2019). The Potential of Elephant Grass (Pennisetum Purpureum Schum), a Nigerian Indigenous Grass, in Bioethanol Production: A Decarbonization Alternative for the Maritime Industry. Southern African Transport Conference.
6. Balan, V. (2014). Current challenges in commercially producing biofuels from lignocellulosic biomass. *International Scholarly Research Notices*, *2014*(1), 463074.
7. Cardoso, J. A., Pineda, M., Jiménez, J. D. L. C., Vergara, M. F., & Rao, I. M. (2015). Contrasting strategies to cope with drought conditions by two tropical forage C4 grasses. *AoB Plants*, *7*, plv107.
8. Chiluwal, A., Singh, H. P., Sahoo, K., Paudel, R., Whithead, W. F., & Singh, B. P. (2019). Napiergrass has dual use as biofuel feedstock and animal fodder. *Agronomy Journal*, *111*(4), 1752-1759.
9. Dien, B. S., Anderson, W. F., Cheng, M. H., Knoll, J. E., Lamb, M., O’Bryan, P. J., ... & Slininger, P. J. (2020). Field productivities of napier grass for production of sugars and ethanol. *ACS Sustainable Chemistry & Engineering*, *8*(4), 2052-2060.
10. Dussadee, N., Ramaraj, R., & Cheunbarn, T. (2017). Biotechnological application of sustainable biogas production through dry anaerobic digestion of Napier grass. *3 Biotech*, *7*, 1-9.
11. Hattori, T., & Morita, S. (2010). Energy crops for sustainable bioethanol production; which, where and how?. *Plant Production Science*, *13*(3), 221-234.
12. Mwendia, S. W., Yunusa, I. A. M., Whalley, R. D. B., Sindel, B. M., Kenney, D., & Kariuki, I. W. (2013). Use of plant water relations to assess forage quality and growth for two cultivars of Napier grass (Pennisetum purpureum) subjected to different levels of soil water supply and temperature regimes. *Crop and Pasture Science*, *64*(10), 1008-1019.
13. Negawo, A. T., Teshome, A., Kumar, A., Hanson, J., & Jones, C. S. (2017). Opportunities for Napier grass (Pennisetum purpureum) improvement using molecular genetics. *Agronomy*, *7*(2), 28.
14. Nyambati, E. M., Muyekho, F. N., Onginjo, E., & Lusweti, C. M. (2010). Production, characterization and nutritional quality of Napier grass [Pennisetum purpureum (Schum.)] cultivars in Western Kenya. *African Journal of Plant Science*, *4*(12), 496-502.
15. Pensri, B., Aggarangsi, P., Chaiyaso, T., & Chandet, N. (2016). Potential of fermentable sugar production from Napier cv. Pakchong 1 grass residue as a substrate to produce bioethanol. *Energy Procedia*, *89*, 428-436.
16. Prapinagsorn, W., Sittijunda, S., & Reungsang, A. (2017). Co-digestion of napier grass and its silage with cow dung for methane production. *Energies*, *10*(10), 1654.
17. Purbajanti, E. D., Anwar, S., Wydiati, F. K., & Kusmiyati, F. (2012). Drought stress effect on morphology characters, water use efficiency, growth and yield of guinea and napier grasses. *Int. Res. J. Plant Sci*, *3*(4), 47-53.
18. Restiawaty, E., Gani, K. P., Dewi, A., Arina, L. A., Kurniawati, K. I., Budhi, Y. W., & Akhmaloka, A. (2020). Bioethanol production from sugarcane bagasse using neurospora intermedia in an airlift bioreactor. *International Journal of Renewable Energy Development*, *9*(2), 247.
19. Samson, R., Mani, S., Boddey, R., Sokhansanj, S., Quesada, D., Urquiaga, S., ... & Ho Lem, C. (2005). The potential of C4 perennial grasses for developing a global BIOHEAT industry. *Bpts*, *24*(5-6), 461-495.
20. Taylor, S. H., Ripley, B. S., Woodward, F. I., & Osborne, C. P. (2011). Drought limitation of photosynthesis differs between C3 and C4 grass species in a comparative experiment. *Plant, cell & environment*, *34*(1), 65-75.
21. Banka, A., Komolwanich, T., & Wongkasemjit, S. (2015). Potential Thai grasses for bioethanol production. *Cellulose*, *22*, 9-29.
22. Cotana, F., Cavalaglio, G., Gelosia, M., Coccia, V., Petrozzi, A., Ingles, D., & Pompili, E. (2015). A comparison between SHF and SSSF processes from cardoon for ethanol production. *Industrial Crops and Products*, *69*, 424-432.
23. Dahnum, D., Tasum, S. O., Triwahyuni, E., Nurdin, M., & Abimanyu, H. (2015). Comparison of SHF and SSF processes using enzyme and dry yeast for optimization of bioethanol production from empty fruit bunch. *Energy Procedia*, *68*, 107-116.
24. Gusakov, A. V. (2011). Alternatives to Trichoderma reesei in biofuel production. *Trends in biotechnology*, *29*(9), 419-425.
25. Kongkeitkajorn, M. B., Sae-Kuay, C., & Reungsang, A. (2020). Evaluation of napier grass for bioethanol production through a fermentation process. *Processes*, *8*(5), 567.
26. Kusmiyati, K., Hadiyanto, H., & Kusumadewi, I. (2016). Bioethanol production from iles-iles (Amorphopallus campanulatus) flour by fermentation using zymomonas mobilis. *International Journal of Renewable Energy Development*, *5*(1), 9-14.
27. Loaces, I., Schein, S., & Noya, F. (2017). Ethanol production by Escherichia coli from Arundo donax biomass under SSF, SHF or CBP process configurations and in situ production of a multifunctional glucanase and xylanase. *Bioresource technology*, *224*, 307-313.
28. Sanford, G. R., Oates, L. G., Roley, S. S., Duncan, D. S., Jackson, R. D., Robertson, G. P., & Thelen, K. D. (2017). Biomass production a stronger driver of cellulosic ethanol yield than biomass quality. *Agronomy Journal*, *109*(5), 1911-1922.
29. Sawasdee, V., & Pisutpaisal, N. (2014). Feasibility of biogas production from Napier grass. *Energy Procedia*, *61*, 1229-1233.
30. Sudiyani, Y., Triwahyuni, E., Muryanto, M., Burhani, D., Waluyo, J., Sulaswaty, A., & Abimanyu, H. (2016). Alkaline pretreatment of sweet sorghum bagasse for bioethanol production. *International Journal of Renewable Energy Development*, *5*(2), 113..
31. Wingren, A., Galbe, M., & Zacchi, G. (2003). Techno‐economic evaluation of producing ethanol from softwood: Comparison of SSF and SHF and identification of bottlenecks. *Biotechnology progress*, *19*(4), 1109-1117.
32. Xu, Q., Himmel, M. E., & Singh, A. (2015). Production of ethanol from engineered Trichoderma reesei. In *Direct microbial conversion of biomass to advanced biofuels* (pp. 197-208). Elsevier.
33. Md Said, M. S., Wan Abdul Karim Ghani, W. A., Hong Boon, T., Hussain, S. A., & Ng, D. K. S. (2019). Thermochemical conversion of Napier grass for production of renewable syngas. *Processes*, *7*(10), 705.
34. Isah Yakub Mohammed, I. Y. M., Yousif Abdalla Abakr, Y. A. A., Feroz Kabir Kazi, F. K. K., Suzana Yusuf, S. Y., Ibraheem Alshareef, I. A., & Chin SohAik, C. S. (2015). Pyrolysis of Napier grass in a fixed bed reactor: effect of operating conditions on product yields and characteristics.
35. Treedet, W., Suntivarakorn, R., Mufandi, I., & Singbua, P. (2020). Bio-oil production from Napier grass using a pyrolysis process: Comparison of energy conversion and production cost between bio-oil and other biofuels. *Int. Energy J*, *20*(2), 155-168.
36. Campos, B. B., Diniz, R. H., Silveira, F. A. D., Ribeiro, J. I., Fietto, L. G., Machado, J. C., & Silveira, W. B. D. (2019). Elephant grass (Pennisetum purpureum Schumach) is a promising feedstock for ethanol production by the thermotolerant yeast Kluyveromyces marxianus CCT 7735. *Brazilian Journal of Chemical Engineering*, *36*, 43-49.
37. Tsai, M. H., Lee, W. C., Kuan, W. C., Sirisansaneeyakul, S., & Savarajara, A. (2018). Evaluation of different pretreatments of Napier grass for enzymatic saccharification and ethanol production. *Energy Science & Engineering*, *6*(6), 683-692.
38. Divyabharathi, R., & Venkatachalam, P. (2015). Energy conversion study on cumbu napier CO− 4. *International Journal of Agriculture, Environment and Biotechnology*, *8*(3), 727-733.
39. Mohammed, I. Y., Abakr, Y. A., Yusup, S., & Kazi, F. K. (2017). Valorization of Napier grass via intermediate pyrolysis: Optimization using response surface methodology and pyrolysis products characterization. *Journal of Cleaner Production*, *142*, 1848-1866.
40. Pensri, B., Aggarangsi, P., Chaiyaso, T., & Chandet, N. (2016). Potential of fermentable sugar production from Napier cv. Pakchong 1 grass residue as a substrate to produce bioethanol. *Energy Procedia*, *89*, 428-436.
41. Singh, B. P., Singh, H. P., & Obeng, E. (2013). Elephantgrass. In *Biofuel crops: production, physiology and genetics* (pp. 271-291). Wallingford UK: CABI.
42. Faleiro, F. G., Kannan, B., & Altpeter, F. (2016). Regeneration of fertile, hexaploid, interspecific hybrids of elephantgrass and pearl millet following treatment of embryogenic calli with antimitotic agents. *Plant Cell, Tissue and Organ Culture (PCTOC)*, *124*, 57-67.
43. Van De Wouw, M., Hanson, J., & Leuthi, S. (1999). Morphological and argonomic characterisation of a collection of napier grass (Pennisetum purpureum) and P. purpureum x P. glaucum. *Tropical grasslands*, *33*(3), 150-158.
44. Wanjala, B. W., Obonyo, M., Wachira, F. N., Muchugi, A., Mulaa, M., Harvey, J., ... & Hanson, J. (2013). Genetic diversity in Napier grass (Pennisetum purpureum) cultivars: implications for breeding and conservation. *AoB Plants*, *5*, plt022.
45. Sattler, S. E., Funnell-Harris, D. L., & Pedersen, J. F. (2010). Brown midrib mutations and their importance to the utilization of maize, sorghum, and pearl millet lignocellulosic tissues. *Plant Science*, *178*(3), 229-238.
46. Hatfield, R. D., Rancour, D. M., & Marita, J. M. (2017). Grass cell walls: a story of cross-linking. *Frontiers in plant science*, *7*, 2056.
47. Mwendia, S. W., Wanyoike, M., Wahome, R. G., & Mwangi, D. M. (2007). Effect of napier head smut disease on napier yields and the disease coping strategies in farming systems in central Kenya. *Livestock Research for Rural Development*, *19*(8), 109.
48. Khan, Z. R., Midega, C. A. O., Nyang'au, I. M., Murage, A., Pittchar, J., Agutu, L. O., ... & Pickett, J. A. (2014). Farmers' knowledge and perceptions of the stunting disease of Napier grass in Western Kenya. *Plant Pathology*, *63*(6), 1426-1435.
49. Farrell, G., Simons, S. A., & Hillocks, R. J. (2002). Pests, diseases and weeds of Napier grass, Pennisetum purpureum: A review. *International Journal of Pest Management*, *48*(1), 39-48.
50. Anderson, W. F., Dien, B. S., Brandon, S. K., & Peterson, J. D. (2008). Assessment of bermudagrass and bunch grasses as feedstock for conversion to ethanol. In *Biotechnology for Fuels and Chemicals: Proceedings of the Twenty-Ninth Symposium on Biotechnology for Fuels and Chemicals Held April 29–May 2, 2007, in Denver, Colorado* (pp. 13-21). Humana Press.
51. Amin, R., Sarker, N. R., Ali, M. Y., Hashem, M. A., & Khatun, M. (2016). Study on cutting intervals on biomass yield, nutritive value and their oxalate content of different high yielding napier (P. purpureum) cultivars. *Asian-Australasian Journal of Bioscience and Biotechnology*, *1*(1), 100-107.
52. Halim, R. A., Shampazuraini, S., & Idris, A. B. (2013). Yield and nutritive quality of nine Napier grass varieties in Malaysia.
53. Macoon, B., Sollenberger, L. E., & Moore, J. E. (2002). Defoliation effects on persistence and productivity of four Pennisetum spp. genotypes. *Agronomy Journal*, *94*(3), 541-548.
54. Yang, Y., Tilman, D., Furey, G., & Lehman, C. (2019). Soil carbon sequestration accelerated by restoration of grassland biodiversity. *Nature communications*, *10*(1), 718.
55. Reddy, K. R., Gomes, V. G., & Hassan, M. (2014). Carbon functionalized TiO2 nanofibers for high efficiency photocatalysis. *Materials Research Express*, *1*(1), 015012.
56. Kommula, V. P., Reddy, K. O., Shukla, M., Marwala, T., & Rajulu, A. V. (2013). Physico-chemical, tensile, and thermal characterization of Napier grass (native African) fiber strands. *International Journal of Polymer Analysis and Characterization*, *18*(4), 303-314.
57. Le Quéré, C., Andrew, R. M., Friedlingstein, P., Sitch, S., Hauck, J., Pongratz, J., ... & Zheng, B. (2018). Global carbon budget 2018. *Earth System Science Data*, *10*(4), 2141-2194.
58. Bujang, M. A., & Adnan, T. H. (2016). Requirements for minimum sample size for sensitivity and specificity analysis. *Journal of clinical and diagnostic research: JCDR*, *10*(10), YE01.
59. Lee, J. W., Kidder, M., Evans, B. R., Paik, S., Buchanan Iii, A. C., Garten, C. T., & Brown, R. C. (2010). Characterization of biochars produced from cornstovers for soil amendment. *Environmental science & technology*, *44*(20), 7970-7974.
60. Hlavsová, A., Corsaro, A., Raclavská, H., Juchelková, D., Škrobánková, H., & Frydrych, J. (2014). Syngas production from pyrolysis of nine composts obtained from nonhybrid and hybrid perennial grasses. *The scientific world journal*, *2014*(1), 723092.